|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Job Information** | | *Item Summary* |  |  |
| **Job Name** | 1095040 - NDSU Engineering Building 2024 | | **Date** | 7/28/2025 |
| **Model** | CAH013GDCM | | **Software Version** | 13.63 |
| **Unit Tag** | AHU-E2 | | | |

| Unit Options |
| --- |

| **Code Item** | **Code Value** | **Description** | List Price |
| --- | --- | --- | --- |
| 1 |  | None | $.00 |
| 2 |  | No Quick Ship | $.00 |
| 3 |  | UNIT CONFIGURATION; Inline horizontal | $.00 |
| 4 |  | DRIVE (HANDING) LOCATION; Right | $.00 |
| 5 |  | EXTERNAL H X W; 48" x 60" | $.00 |
| 6 |  | SHIPPING SECTION CABINETRY | $20,500.33 |
| 7 |  | CASING DETAILS | $.00 |
| 8 |  | OUTER PANEL; 24 gauge G90 galv steel (unpainted) | $.00 |
| 9 |  | LINER; 24 gauge Galvanized steel | $.00 |
| 10 |  | INSULATION; R-13 Injected Foam | $.00 |
| 11 |  | FRAME; 2.00" | $.00 |
| 12 |  | SHIPPING PROTECTION; None | $.00 |
| 13 |  | 6" STANDARD BASERAIL (COMPLETE UNIT) | $4,568.45 |
| 14 |  | MIXING BOX SECTION (SHIP SECTION #1) | $.00 |
| 15 |  | DAMPER TYPE; Parallel blade | $1,497.18 |
| 16 |  | LOCATIONS; End, Top | $.00 |
| 17 |  | DOOR (WIDTH); Drive side (28.0") | $.00 |
| 18 |  | HD FLOOR LINER; Galvanized steel | $.00 |
| 19 |  | LIGHT KIT; LED marine light kit and switch only | $310.54 |
| 20 |  | FILTER DATA | $.00 |
| 21 |  | WITHDRAWAL; Side | $704.57 |
| 22 |  | STYLE; Angular | $.00 |
| 23 |  | TYPE; 4" Pre Pleat (MERV 13) | $590.37 |
| 24 |  | GAUGE; Magnehelic 0-2" | $386.52 |
| 25 |  | DOOR (WIDTH); Drive side (0.0") | $.00 |
| 26 |  | LIGHT KIT; LED marine light kit and switch only | $.00 |
| 27 |  | COMBINATION COOLING COIL & REHEAT COIL SECTION (SHIP SECTION #2) | $.00 |
| 28 |  | CHILLED WATER COIL | $544.35 |
| 29 |  | COIL MODEL; 5WH1205B0390004700HRHVCGCCE35TC017A7ST1000C001000C0001000100YYYAYYYYYYYYYYYYYYYYYYYYYYYYYY | $7,671.40 |
| 30 |  | QTY; 1 | $.00 |
| 31 |  | COIL SIZE; Large | $.00 |
| 32 |  | REHEAT HOT WATER COIL | $345.07 |
| 33 |  | COIL MODEL; 5WH1002C0390004400HRHVCGCHE35TC017A7ST1000C001000C0001000100YYYAYYYYYYYYYYYYYYYYYYYYYYYYYY | $4,287.22 |
| 34 |  | QTY; 1 | $.00 |
| 35 |  | COIL SIZE; Large | $.00 |
| 36 |  | DRAIN PAN; Stainless steel | $1,222.74 |
| 37 |  | HD FLOOR LINER; Galvanized steel | $.00 |
| 38 |  | ACCESS SECTION (SHIP SECTION #3) | $.00 |
| 39 |  | DOOR (WIDTH); Drive side (14.0") | $.00 |
| 40 |  | WINDOW; Round | $.00 |
| 41 |  | HD FLOOR LINER; Galvanized steel | $.00 |
| 42 |  | LIGHT KIT; LED marine light kit and switch only | $310.54 |
| 43 |  | SUPPLY FAN SECTION (SHIP SECTION #4) | $.00 |
| 44 |  | FAN TYPE; SISW | $8,913.25 |
| 45 |  | WHEEL TYPE; EC355 Class II | $.00 |
| 46 |  | DISCHARGE LOCATION; Axial | $.00 |
| 47 |  | MOTOR HP; 3.45 HP, Open drip proof, Premium efficiency, 200/60/3, 3230 RPM | $.00 |
| 48 |  | DRIVE TYPE; N/A, service factor=0.00 | $.00 |
| 49 |  | BEARING TYPE; N/A | $.00 |
| 50 |  | ISOLATOR TYPE; Rigid | $.00 |
| 51 |  | VFD/STARTER/DISCONNECT | $.00 |
| 52 |  | ; Starter | $1,121.65 |
| 53 |  | DOOR (WIDTH); Removable panels (20.0") | $.00 |
| 54 |  | HD FLOOR LINER; Galvanized steel | $.00 |
| 55 |  | PLENUM SECTION (SHIP SECTION #5) | $.00 |
| 56 |  | OPENING LOCATION; Top | $.00 |
| 57 |  | DOOR (WIDTH); Drive side (18.0") | $.00 |
| 58 |  | WINDOW; Round | $.00 |
| 59 |  | HD FLOOR LINER; Tread plate | $.00 |
|  |  | List Each: | $52,974.19 |
|  |  | Quantity: | x 1 |
|  |  | Total Ext List: | $52,974.19 |